Lab Manual

# Data Communication Networks

**BCA324 III**

**NAME: SUJAL KHUNT**

**ENROLLMENT NO:** **24FOTCA13902**

**TUTORIAL : 5**

# 1.Using Command Prompt

Press Win + R to open the Run dialog.

Type cod and press Enter to open Command Prompt.

Type ipconfig and press Enter.

Look for the "Ethernet adapter" or "Wireless LAN adapter" secBon, depending on your connecBon type. The IP address will be listed under "IPv6 Address."

# Using Se=ngs

Open the Start menu and go to SeKngs (or press Win + I).

Go to Network & Internet.

Click on Status from the leP pane.

Click on ProperBes under your acBve network connecBon (either Wi-Fi or Ethernet).

Your IP address will be listed under "IPv6 address."

# Using PowerShell

Press Win + X and select Windows PowerShell or Windows Terminal.

Type Get-Enfilades and press Enter.

Look for the secBon related to your network adapter. The IP address will be displayed under the IP Address column.